Details to discharge condition 3 of Listed Building Consent Application 23/00715/LBC
Please find details of the windows we are proposing to install as the planning permission requested details to be provided. 
D1 - Kitchen door
[bookmark: _GoBack]W1 - Bedroom window 
W2 - Dining room window
W3 - Bathroom window 
W4 - Kitchen window adjacent door. 
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W3 @ 1100w x 1060h Bespoke TRO21 with 320mm
transom. pine Trentham Stormproof White Primed
window, 70mm Projecting Cill, Black gasket and
chrome furniture, 2 x 24mm D/G obscure (autumn
leaf) panes (with black warm edge spacers). ***
These frames are 75mm deep front to back ***
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W1 @ 1600w x 1000h Bespoke TRO31 with 320mm
transom and L/H fanlight only. pine Trentham
Stormproof White Primed window, 70mm
Projecting Cill, Black gasket and chrome furniture, 3
x 24mm D/G clear panes (with black warm edge
spacers). *** These frames are 75mm deep front to
back ***
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D1@ 915w x 2170h (815mm x 2070mm door leaf) 3
section mid-railed and panelled door. pine, primed

white, 1 x mid-rail, 1 x bottom vertical muntin, 2 x
flat (tricoya) panels, 1 x 24mm D/G toughened clear
pane (with black warm edge spacers), black gasket,
70mm projecting cill and chrome furniture. open in,
door hung on R/H/S (viewed from outside). *** Door
frames are 95mm deep front to back *** 1 x moon
board @ 1590mm - to be shaped and connected to
D1 & W4 onssite by others ***
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W4 @ 675w x 1190h Bespoke 50/50 TRO21 pine
Trentham Stormproof White Primed window, 70mm
Projecting Cill, Black gasket and chrome furniture, 2
x 24mm D/G Toughened clear panes (with black
warm edge spacers). *** These frames are 75mm
deep front to back ***
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W2 @ 2125w x 1000h Bespoke window with
360mm transom. pine Trentham Stormproof White
Primed window,70mm Projecting Cill, Black gasket.
1x 24mm D/G Toughened clear pane in bottom and
3 x 24mm D/G clear panes (with black warm edge
spacers). *** These frames are 75mm deep front to
back *** 1 x moon board - to be shaped and
connected on site by others ***




