Baildon Road Condition Discharges

Condition 4 
  Rear properties will have a blocked paved patio area, 2m x 4m in area to allow surface water to drain through the pavers with each property having a rain water gully to take any excess  from the patio area with water butts to take rain water from the downspouts for harvesting. United Utilities have approved all drainage plans and water harvesting measures.

Condition 5
Level plans are attached

Condition 6
Bird Table image supplied
Resin specification is attached
All doors and windows will be UPVC Grey manufactured by VEKA. Link attached

Condition 7

Window and door reveal plan attached
