Proposed Landscaping 
Ref: SR.141124.A
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Lawned area  
•	All planting operations shall comply with BS 4428 (1989) & AMD, Code of Practice for General Landscaping Operations
•	Total minimum soil depths: 150 mm topsoil, minimum 450 mm subsoil 
•	Subsoil shall conform to BS 8601:2013 Specification for Subsoil and             requirements for use.
•	Topsoil conforming to B.S. 3882: 2015 shall be multi-purpose soil of uniform composition throughout, of light to medium texture, and shall be capable of being broken down to a fine tilth.
•	Lawn with rye grass mix shall be: 
PM51 Greenscape by Olivers seed www.oliver-seeds.co.uk or similar comprising: 
40% Double, 4turf tetraploid ryegrass 
30% Maxima, Strongcreeping red fescue 
30% Esquire, Perennial ryegrass
•	Sowing rate: seed at a rate of 35 – 50 g per m2 
Hedge planting
Hedge planting as shown on the plan and on the inside of the 1.5m stone boundary wall. 

Whip planting details
	%
	Botanic
	Common
	Nursery size

	50
	Crataegus monogyna
	Hawthorn
	Min 750mm 

	50
	Prunus spinosa
	Blackthorn
	Min 750 mm



Planting to be in two rows 1 metre apart and at 0.75 metre centres, staggered.
Maintenance
Any plants failing within first 5 years to be replaced by same
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