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Specification

Brand Forest Garden
Cladding Overlap
1952nm —— 868 —— Cladding Thickness 7mm/028inch
; | C - Construction Type Overlap
Depth at Base 750mm /2 eet 553 inches
e - Depth including Overhang. 868mm /2 feet 10,17 inches
Door Height 1252mm/ 4feet 129 inch
Door Type Double Doors
-2 Door Width 760mm/ 2 feet 5.92 inches
- 6w ———— = T50nm —— Framing Size 28x28mm
Size &x2
Guarantee 15years
Locking System Haspand Staple
Packaged Weight 6835kes
Ridge Height 1455 mm/ 4 feet 9.28 inches
Roof Covering GreenSand Felt
Roof Material 0SB (Oriented Strand Board)
Roof Thickness 8mm/031inch
Roof Style Pent
Material Wooden
Treatment Pressuretreated

Width at Base 1828 mm /5 feet 11.97 inches
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