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Figure 2 Default spedification for protective barrier
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1 standard scaffold poles

2 Hemvy gauge 2 m all galanized tube and welded mesh infil pancls
3 panels secured to uprights and cross-members with vire ties

4 Ground level

5 Uprights criven into the ground unti secure (minimum depth 0.6 m)
& Standard scafold clamps
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Figure 3 Examples of above-ground stabilizing systems

b) Stabilizer strut mounted on block tray





