
SUSTAINABLE DRAINAGE AND LANDSCAPE MANAGEMENT PLAN FOR FORMER CASTLETON SIDINGS, ROCHDALE  

1.0  An introduction to sustainable drainage systems or SuDS
SuDS are a new environmentally friendly approach to managing rainfall that uses landscape features to deal with surface water. SuDS aim to:
· Control the flow, volume and frequency of water leaving a development area
· Prevent pollution by intercepting silt and cleaning runoff from hard surfaces
· Provide attractive surroundings for the community
· Create opportunities for wildlife


2.0  SuDS at Castleton Sidings, Rochdale. 
The site is a brownfield site, which originally drained unattenuated into an existing culvert, which in turns outfalls into Trub Brook to the south of the site.
Unfortunately due to the underlying ground conditions soakaways are not suitable for this site.
Through negotiation with Rochdale Council’s LLFA the surface water discharge rate was agreed to be restricted to 90l/s for the 1 in 100 year event (plus 45% climate change). The storage will be held in oversized pipes and an online storage crate. 
In the same email the LLFA advised at the time that a pond would be less expensive than buried tanks, but would ‘leave the details to ourselves’, therefore to maximize usable public open space underground storage crates are required. (See Appendix A)

3.0  Managing the SuDS / Landscaped areas
The underground storage crates and landscaped areas have been designed for easy maintenance to comprise:
The Plan contained in Appendix B shows the areas to be maintained by the proposed Management Company have been coloured blue and green on the plan, with the pink areas being either maintained by the residents or Rochdale Councils Highways Department.
The Sewers shown coloured Red and Blue on the Section 104 Plan contained in Appendix C will be adopted by Murphy Group once the site has completed and following a 12month maintenance period and Kellen Homes have completed any remedial works required by Murphy Group.


Kellen Homes will undertake all maintenance works until such time the areas are adopted.
These works will include the following:
· Regular “day to day” care - litter collection, grass cutting and checking silt traps, inlets and outlets where water enters or leaves a SuDS feature.
· Occasional tasks - managing vegetation and removing any silt that builds up in the SuDS features
· Remedial work - repairing damage where necessary

4.0  Spillage – EMERGENCY ACTION

Most spillages on development sites are of compounds that do not pose a serious risk to the environment if they enter the drainage in a slow and controlled manner with time available for natural breakdown in a treatment system. 
Therefore small spillages of oil, or other known organic substances should be removed where possible using soak mats as recommended by the Environment Agency with residual spillage allowed to bio-remediate in the drainage system.
In the event of a serious spillage, either by volume or of unknown or toxic compounds, then isolate the spillage with soil, turf or fabric and block outlet pipes from chamber(s) downstream of the spillage with a bung(s). (A bung for blocking pipes may be made by wrapping soil or turf in a plastic sheet or close woven fabric.)
Contact the Environment Agency immediately.

5.0  Existing Culvert.

The existing culvert shown by a green line on the Management Plan contained within Appendix B will be maintained by the Management Company. (A copy of Trustgreen’s Order Confirmation is included in Appendix E). 
Trustgreen’s offer states that the culvert will be inspected in accordance with CIRIA Guidance.
Appendix F contains a “Maintenance Regime for Culverts / Pipes” (Based on CIRIA C689 – Culvert Design and Operation Guide)
The route is protected by an easement preventing home owners from building over the culvert. A copy of the  “Overall Plot Deed Plan” is contained within Appendix D.
The culvert is shown on the approved Section 38 Drawings. Rochdale Highways Department have granted Section 38 Technical Approval for the drawings listed in the Planning Decision Notice, a copy of the confirmation is contained in Appendix A





5.0 Typical SuDS and Landscape Maintenance – Summary

	
	Frequency

	
	REGULAR MAINTENANCE
	

	1
	LITTER MANAGEMENT
	

	1.1
	Pick up all litter in SuDS and Landscape areas and remove from site
	12 visits monthly

	
	
	

	2
	GRASS MAINTENANCE – all cuttings to wildlife piles
	

	2.1
	Mow all grass verges, paths and amenity at 35-50mm with 75mm max. Leaving grass in situ
	As required or monthly

	2.2
	Mow all dry swales, dry SuDS basins and margins to low flow channels and other SuDS features at 100mm with 150mm max. Cut wet swales or basins annually as wildflower areas
	4-8 visits as required Annually

	2.3
	Wildflower areas strimmed to 50mm in Sept or at end of school holidays
Or
Wildflower areas strimmed to 50mm on 3 year rotation 30% each year
	1 visit annually



1 visit annually

	
	
	

	3
	INLETS AND OUTLETS
	

	3.1
	Inspect monthly, remove silt from slab aprons and debris. Strim 1m round for access if required.
	4 visits yearly

	4
	WETLAND AND POND VEGETATION
	

	4.1
	Wetland vegetation to be cut at 100mm on 3 – 5 year rotation. 30% each year. All cuttings to be removed to wildlife piles or from site.
	As required

	
	
	

	5
	SILT MANAGEMENT
	

	5.1
	Inspect crates, swales, ponds and wetlands annually for silt accumulation
	4 visits yearly

	5.2
	Excavate and remove silt
	As required

	5.3
	[bookmark: _Hlk199769566]The existing culvert will be maintained by the Management Company (a copy of Trustgreen’s Order Confirmation is included in Appendix E). Within their quotation it refers inspections to “CIRIA Guidance”.
Appendix F contains a “Maintenance Regime for Culverts / Pipes” (Based on CIRIA C689)
	1 visit annually

	
	
	

	6
	REMEDIAL WORK
	

	6.1
	Inspect SuDS system regularly to check for damage or failure.
Undertake remedial work as required.
	As Required

	5.3
	Existing Culvert – the culvert will be maintained by the management company. Undertake remedial work as required.

	As Required
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APPENDIX A – Technical Approvals

1.0 - Discharge Rate Approval 
[image: A email with text and images
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APPENDIX A (cont.)

2.0 -  Section 38 Technical Approval 



APPENDIX B
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Management Company Plan

APPENDIX C
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APPENDIX C (cont)
[image: A map of a neighborhood

AI-generated content may be incorrect.]
APPENDIX D
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Overall Plot Deed Plan
APPENDIX E








APPENDIX F
Synopsis: Maintenance Regime for Culverts / Pipes (Based on CIRIA C689)
Objective:
To ensure culverted watercourses remain effective and safe, preventing blockages, flooding, and structural failure through a proactive maintenance regime.
Maintenance Regime Overview
CIRIA C689 emphasises a risk-based maintenance approach tailored to the culvert’s location, design, catchment characteristics, and downstream sensitivity. Maintenance should include inspection, cleaning, vegetation control, debris removal, and structural assessment.
Recommended Timescales for Maintenance Activities
	Activity
	Recommended Frequency
	Notes

	Routine Visual Inspections
	Annually 
(typically in spring/autumn)
	Adjust frequency based on debris load and risk level.

	After Major Storm Events
	Within 24–72 hours post-event
	Essential to assess for blockage or structural impact.

	Debris and Sediment Removal
	Annually based on inspection
	More frequent in urban/high-debris catchments.

	Vegetation Management (at inlets / outlets)
	Annually or as required
	Prevents root intrusion and flow obstruction.

	Structural Inspection
	Every 5–10 years (detailed survey)
	Align with asset management planning cycles.


Key Considerations
· Maintenance frequency must be adaptive based on performance records and environmental changes.
· Implementing a culvert asset management register supports scheduling and tracking.
· Use remote monitoring (e.g., cameras or telemetry) in inaccessible or high-risk locations for early warning.
Conclusion
A structured maintenance regime with well-defined timescales based on CIRIA C689 helps reduce flood risk, prolong culvert life, and support regulatory compliance. The timescales should be reviewed periodically and adjusted as needed based on asset condition and catchment dynamics.
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1ohn Gilighan WN <johngilighan@rochdale gov.uk>
08 November 2024 1009

Lewis Shaw

RE 23147 - Heywood Road, Casteton, Secion 38 Application
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CAUTION: This email originated from outside your organisation. Exercise caution when openi
attachments or clicking links,especally from unknown senders.

Lowis,
Ves you have Technical Approvl,

Thanks,

John Gillighan WN

‘Sanior Engineer (Highways)

Network Improvement & Development

2 ROCHDALE

BOROUGH COUNCIL

R 01706 924607
3 john.gilighan@rochdale gov.uk
Rochdale Borough Council

Floor 2, Number One Riverside
‘Smith Street, Rochdale, OL16 1XU

o access our services go to waw.rochdale gov.uk
For news, events and social media updates go t /. rochdale gov.uklnewsandevents

nvironment before printing this email

To:John Giighan WN <jonn gilighan@rochdale govuk>
Subject: RE: 23147 - Heywood Road, Castleton, Secion 38 Application

HiJohn,
'Does this mean we have technical approvalor at which point il be confirmed?

Kind ragards
Lowis

Froms John Gilighan WN <iohn ilghan Srochdae gov.u>
Sent: 06 November 2024 1107

Subject: RE: 23147 - Heywood Road, Castleton, Secion 38 Application
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Trustgreen Order Confirmation
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From: Stephen McCann <Stephen McCann@Rochdale Gov.UK>

Sent: 09 July 2021 1224

To: ElannaHerod@campbellreith com; Tom Foster

ce GaryTaylor@campbellreith.com

Subject: RE: QUESTIONS re. Confirmation of future Discharge of rate - to culvert : Castleton,
Rochdale - Discharge Rate Enquiry

Attachments: Land Ownership queries - Castleton Sidings - notes. pdf

Follow Up Flag: Follow up.

Flag Status: Flagged

Hello Elanna and Tom

Hooked at the Campbell Reith CAD drawing of the brownfield areas for the site and I'm happy with your calculation
‘with 30% reduction i.e. SW discharge flow rate of 90 /5 (rounded up from 87.61/5).

‘The design of your proposed vortex control should be for this. 'm not sure what attenuation measures you will
include?

A pond s less expensive than a buried attenuation tank?
One way to reduce runoff i to have some impermeable surfaces for parking areas.
Perhaps there is scope for 2 pond on the southern boundary? However, | leave the details to you.

It's worth noting that Land Registry does not have a known owner for Areas A and B on the appended Plan. Area Cis
the farmer, as you know.

Stephen McCann
Drainage & Flooding Engineer
Highways, Property & Strategic Housing

7 ROCHDALE

BOROUGH COUNCIL

01706 924606

[ o7ss2 570262

(£ stephen.mccann@rochdale.gov.uk
Rochdale Borough Council

Floor 2, Number One Riverside
Smith Street, Rochdale, OL16 1XU

To access our services go to www.rochdale.gov.uk
For news and social media updates o to www.rochdale.gov.ukinews

Please consider the environment before printing this email.
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