PROPOSED REDEVELOPMENT, DEXINE RUBBER WORKLS, SPOTLAND

OUTLINE PLANTING SPECIFICATION 
EXISTING HORNBEAM RENTION & PROTECTION 

The existing Semi mature Hornbeam tree on Spotland Road being located outside the hoarding line of the construction site is to continue to be protected during the works by the retention of the site hoardings until soft landscape works are due to commence on Spotland Road. 

The tree should be inspected by an Arboricultural consultant to check its stability, and health and advise and any necessary tree works.

Any necessary crown lifting or minor pruning works shall take place outside the bird nesting season (1st March to 31st August inclusive), unless the site is surveyed for nesting birds by a qualified ecologist prior to pruning and if any active nests found the work must be delayed until fledglings have flown the nest.
All materials for construction purposes should be stored outside of the canopy and rooting zone of the tree .
All toxic materials such as oils, bitumens and residues from concrete mixing should be kept well away from the protection zone/drainage zone of the trees well away from its root system, and should be retained within effective catchment areas as far away as possible to avoid risk of tree root contamination. The routing of any services within the tree canopy/ root protection zone  should be avoided as far as possible. Any excavation that should prove necessary within the tree canopy and rooting zones eg for proposed fencing posts or drains should be carried out by careful hand dig if necessary to avoid root damage.

EXISTING IVY REMOVAL TO WALLS TO BE DEMOLISHED 
Any Ivy to be removed to the existing brick wall on Primrose Street, shall be removed outside the bird nesting season (1st March to 31st August inclusive),. or if removal prior to then is necessary the Ivy should be checked for nesting birds by a qualified ecologist prior to pruning, and if any active nests found the work must be delayed until fledglings have flown the nest.

TOPSOIL SUPPLY AND DISTRIBUTION TO ALL TREES, SHRUBS, AND GRASS AREAS INCLUDING CAPPING LAYER 

AND TESTING REGIME AS SPECIFIED IN CCG PHASE II GEONINVIRONMENTAL REPORT  

All topsoil to be imported, unless otherwise stated or left in situ. Contractor to allow for all relevant Topsoil Analysis and Certification to be presented prior to imported topsoil supply and delivery to prove that the topsoil  meets BS 3882:2015 Specification for Topsoil and requirements of Multi Purpose Grade, to prove its suitability for trees, shrubs and amenity grass, and to prove that the topsoil is free of contaminants. Imported Topsoil should also preferably be an As Dug ( natural ) topsoil rather than a manufactured topsoil.

All imported topsoil is also to be subject to any necessary testing and validation procedures that TJ Booth may recommend in their latest Phase 1 and 2 or any subsequent Environmental audit, 

 A 600mm depth clean topsoil capping layer in accordance with TJ Booth specifications shall be introduced to all soft landscape areas and shrub beds, inc any geotextile membrane that may be specified beneath the soil.
PROPOSED  TREE PLANTING 
Proposed trees are To be planted in 1.5m  x 1.5m x 600 mm depth pits ( over a porous geotextile membrane if required as [part of remediation requirements) beneath tree pits. Planting medium to pits comprising 80% approved quality clean imported topsoil and  20% approved peat free compost and Enmag fertilizer to be incorporated at a rate of 70 grams/m2. Mycorrhizal fungus should be applied to new tree either in the form of powder, granules or spikes. Powder and granules should be applied over the exposed roots of the transplanted tree and spread over the newly dug hole. Mycorrizal spikes should be pushed into the rootball once the tree has been planted. An irrigation pipe -eg Green -  tech Mona Relief Grande MRG 3 ( 3m x 60mm dia pipe) to be supplied with a Mona Relief Grande Aria Inlet;  or similar approved,  irrigation  pipe & cover to be installed around tree root ball. Trees to be secured by two 100 mm dia. treated softwood stakes pointed at one end. Stakes to be driven into existing ground beneath tree pit 300mm min, with care not to damage the capping separation membrane any more than necessary . Top of stakes to be approx 750mm  above ground, and fixed to tree with a timber cross bar, spacer and rubber tie – type to be agreed. Allow for watering in to field capacity upon planting and then a second watering 48 hours later, and regularly during dry periods. Trees within grass areas are to receive a 800mm dia circle of bark mulch around base. Allow for ventilated clear spiral rabbit guards to base of trees. 

Tree locations on the drawing are indicative- and are to be agreed on site and in liaison with Project coordinater and TJ Booth, particularly in relation to retaining walls and underground services.
ORNAMENTAL SHRUBS & GROUNDCOVER PLANTING 

All proposed shrub and groundcover areas are to potentially receive a 600 mm depth approved quality clean imported topsoil capping layer; ( laid over a geotextile membrane if specified by engineer) , and de-compacted and free draining formation level. To be made weed free, and cultivated, including incorporating a 35mm layer of peat free compost across whole of shrub beds, and incorporating Enmag fertilizer at a rate of 70 g/m2 both to be worked into the full depth of topsoil prior to planting. All plants to be well watered in. Bark mulch to whole of finished shrub beds to be 75mm layer of approved quality coarse/medium grade bark mulch.
GRASSED AREAS TO RESIDENTIAL HOUSES  
Any rear lawns included to the new houses  shall  receive 600mm depth clean topsoil capping layer  ; ( laid over a geotextile membrane if specified by engineer) . To be laid over a de compacted and free draining formation and cultivated, and made weed free and turfed with an approved quality hard wearing shade tolerant cultivated  turf from a reputable supplier. 
GENERAL PLANT SUPPLY & PLANTING
All plant material to be supplied in accordance with BS 8545 " Trees: from nursery to independence in the landscape -Recommendations" BSI 2014; BS 3936 Parts1-4 and 9-10, and B.S. 5326 All plants to the correct species and stock size specified, and to be good specimens characteristic of species. All plants to be supplied free from pest and disease. All indigenous trees and shrub species have been specifically selected for their form, height, & individual characteristics, therefore no substitution of species to be carried out without prior consent. Planting operations are to be carried out during suitable weather avoiding periods when ground is frozen ,waterlogged or excessively dry spells. All trees & plants should be watered in well at time of planting.
STATUTORY SERVICES & DRAINAGE AND TREE PIT EXCAVATIONS
The landscape contractor should establish positions and depths of all drains & services, including any realigned services, on site prior to any ground modelling or excavation works. Any potential conflict with proposed trees  and drains or services should be brought to attention of the Clients Project Coordinator , and realigned positions agreed, or ribbed root directors/ barriers used - to be agreed on site prior to planting. Contractor to allow for tree pits to be hand dug with care to avoid services.
Localised area of drain within car park under/ in immediate vicinity of planting island bed to be laid in concrete as agreed with engineer - to allow a tree to be planted.

OUTLINE MAINTENANCE SPECIFICATION

All soft landscape elements are to be maintained and guaranteed by the landscape contractor during 12 months defects liability period if applicable, and thereafter under a Maintenance regime arranged by the developer. Regular maintenance operations to the new planted areas are to include monthly weeding operations to trees, and shrub areas, and pruning as necessary to promote flowering, form etc. Pruning should be left until late winter to leave seeds and berries for wintering wildlife and to ensure no impact on breeding and nesting birds.

Maintenance visits should also include checking and adjusting tree stakes and ties. Also watering new trees, shrubs and grass areas  as necessary during prolonged dry periods. Also mowing  lawn areas regularly during the growing season ( every 1 to 2 weeks). 
Contractor to allow for  replacing any plant failures, and repairs to grass areas & topping up bark mulch annually to trees and planting beds during establishment period. 
NB  The use of herbicides insecticides and slug pellets should be avoided during maintenance operations to prevent fatal effects on the food chain Any herbicides should be non residual and approved by Environment Agency for use near waterways  in respect to proximity to River Spodden.
OUTLINE IMPLEMENTATION PROGRAMME 

To be agreed by developer but potentially as follows:-

Form new topsoiled shrub beds, and for tree pits , and carry out new shrub planting and turfing during 

late summer / early autumn 2021

Tree planting to be carried out during November 2021 planting season , or if carried out prior to November, trees must be supplied container grown or in Air pots 

All planting works are to be carried out avoiding frozen ground conditions or excessively wet conditions or drought conditions  

