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Drainage Consultation on Application – 25/00195/FUL - 
Land At Schofield Street Heywood OL10 1DH
LLFA Consultation Response on behalf of Head of Highways and Engineering
Date of Response: 21st June 2025
Location & Proposed Development
Land At Schofield Street Heywood OL10 1DH
Residential development consisting of 9no' 4-bedroom dwellings with associated parking and landscaping
Documents Reviewed
· CGI-1. CGI-2. CGI-3, images
· Consultation from United Utilities, dated 8th May 2025
· Existing Site Plan 24.3378.1C
· Proposed Site Plan 24/3378.SC1.1K
· Site Location Plan V2
· PHASE I, II AND III SITE INVESTIGATION, dated January 2025
Drainage & Flood Officer Comments
1. The proposal has not included any drainage information to support the planning application. 
 
2. The aim should be to discharge surface run off as high up the following hierarchy of drainage options as reasonably practicable: The ordered drainage techniques to be assessed with the aim to reduce or omit lower techniques:
· Control at Source (Infiltration / Recycling)
· On Site Treatment (Basins, Swales, Rain gardens, Tree pits)
· Local Treatment (Adoptable Ponds, Basins, Swales etc)
· Regional Treatment (ditto usually to a larger scale)
· Discharge to Watercourses / Bodies
· Discharge to SW Sewers
· Discharge to Combined Sewers

3. The proposal’s design feasibility should be based on a 1-in-100-year storm event with a 45% allowance for climate change, which is appropriate for peak rainfall. This climate allowance is appropriate for the ‘Irwell Management’ Catchment area for ‘More’ vulnerability class.

4. The proposal has included a Phase I, II and III ground investigation. 
The ground investigation report indicates the presence of significant contamination including asbestos and hydrocarbons. The report further advises remediation works. 
Due to the contaminated ground conditions identified in the ground investigation, infiltration-based SuDS may not be suitable for this site. 

5. There are no watercourses or surface water sewers within reasonable proximity to the site.

6. It is assumed that attenuated discharge to combined sewers are the most likely drainage option. Discharge volumes should be mitigated utilizing SuDS green-based source control such as swales, raingardens tree-pits etc. Rainwater harvesting for potable re-usage such as WC flushing could also be considered. 

7. A comprehensive Sustainable Drainage Assessment should be prepared to explore all viable surface water mitigation options and support the future planning application.
· 
Drainage & Flood Officer Summary:
I. A sustainable drainage proposal should be submitted to support the application. 
II. A proposal should be acceptable in principle before any conditions could be considered. 

Consultation by Keith Mealey
Drainage & Flooding Officer
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