Method Statement for 22/01515/LBC proposed reinstatement of four bricked up windows to front elevation.

1. Cut through concrete rendering using an slitting disc on a 110v angle grinder around bricked up windows.
2. Carefully remove rendering from stone mullions and clean.
3. Remove rendering and brickwork to windows leaving openings.
4. Fit new hardwood and painted window frames to match existing windows.
5. Point and make good to outside.
6. Repaint external frames.

Window details
Hardwood and painted casement windows, two pane as per original windows, (see photograph of existing front elevation.
