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Date: 09/04/2025
Team: Environmental Control (Landfill Gas) 
Application Number: 25/00280/DOC 
Proposal: Submission of details to comply with conditions 15 (site investigation), 16 (site investigations-coal), 17 (archaeology), 19 (connections to foul sewer), 20 (surface water drainage), 21 (construction method statement), 22 (construction traffic management plan), 23 (construction environmental management plan), 25 (Landscape and Habitat creation and management plan) and conditions 28 (water main protection) on planning permission 16/01399/HYBR

Dear Nick, 

I have read the document submitted by the applicant (WSP Ref. No. 70114074-GIR-003.  I am in agreement with the conclusions.  Namely:

Whilst specific remedial measures are not required in relation to soil contamination, development site staff need to be aware that contamination could be uncovered during ground works. The steps to follow if such contamination is encountered should be outlined in a remediation strategy, which will be subject to regulatory approval.
The potential for ground gas accumulation within excavations during construction will need to be considered and addressed with appropriate monitoring / protective equipment.
Full radon protection measures will need to be installed in new structures. The requirements will need to be outlined in the remediation strategy and the measures designed by a specialist.
Hazardous ground gas protection measures are also required in new structures (Characteristic Situation 3). It is considered that the full radon protective measures would likely mitigate provide the required level of protection. Hazardous ground gas and radon protection measures need to be specified in the remediation strategy and designed by a specialist.
The installation of ground gas / radon mitigation will need to be validated by an independent and suitably qualified party, in accordance with the requirements laid out in the remediation strategy.
It would be prudent to complete a water pipeline assessment to ascertain the need for barrier pipe if new potable water pipes will be laid in existing Made Ground. Once the route of potable water pipes is known the information within this report should be reviewed and a UK WIR pipeline assessment completed if required.
A hazardous waste assessment will be required if the mounded Made Ground is to be taken offsite to landfill. If the material is to be used elsewhere within the development, it is recommended that this is undertaken in accordance with a CL:AIRE Definition of Waste Code of Practice-compliant materials management plan.
Re-use of site won materials should be managed through the preparation of a Materials
Management Plan (MMP)

I should also note that one of the documents referenced within this report (BRE211) was updated in 2023 (the 2015 version is referenced within the report).  Any radon protection measures require to be designed in accordance with the 2023 version.

A remediation strategy will be required.  Therefore, at this time, condition 9 within 16/01399/HYBR should not be discharged in its entirety, but condition 9 (i) may be discharged if you are so inclined.

Yours sincerely,

Jonathon Parr

Jonathon Parr
Environmental Health Senior Officer (Environment Prot)
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