[Type here]

discharge condition 3 (materials) of planning permission 20/01333/FUL


1. Material (e.g. Brick)

· Location of material (i.e. Elevations)   - brick is to all elevations approx. 2100mm from floor level
· Colour-  red engineering brick
· Texture- smooth
· Image- attached
· Product link   https://dam-assets.apps.travisperkins.group/xdm5eg3/wienerberger-class-b-red-perforated-engineering-brick-65-mm-pack-of-504~GPID_1000327683_TECH_00.pdf

2. Material (e.g. cladding)

· [bookmark: _GoBack]Location of material   cladding to all elevations above brick level front is cladded in trimapanel 
· Colour -  Goosewing grey
· Texture -  textured
· Image - attached
· Product link-  https://www.tatasteeluk.com/sites/default/files/trimapanel%C2%AE-fw-datasheet.pdf  


