Plaque Size & Fixing Details

The estimated size of the plaque would be:  460 X 350 mm ( portrait format.)
In terms of the fixing I would write words to the effect in my method statement as part of the application:

“ The bronze plaque would have a hollow back ie. it is cast from 4-7 mm thick metal.  It will have a 5mm hole in each of the corners of the plaque.  The exact position of these would correspond with the bed or perpendicular mortar joints in the masonry.  

The fabric of the building in the fixing location would be surveyed at the design period to ensure that the position of the fixings would be woven into the design of the overall plaque at the earliest stage thus ensuring that the stone ashlar would not be disturbed in any way.  Furthermore it would be possible for the plaque to be removed at some point in the future without any damage to this stonework.

The plaque would be dry fixed to the wall with the following method:

Holes 1 mm smaller than the thickness of the mortar joints would be drilled and a plastic plug with a dovetailed rear section ( to prevent the removal of these fixings by force ) would be placed into the holes recessed by 1mm.
Four brass tamperproof screws would fix the plaque onto the wall without the need for mortar or resin joints."

