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Solar PV Project – Prior Approval Planning Information
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Description automatically generated]Bowlee Primary School
Prior Approval Supporting Information

Date completed; 13th Oct 2025 	Amended: 13th Oct 2025 



	Site Address:
	Windemere Road, Middleton, M24 4LA


	Solar PV Installation Overview
	138.86 kWp installation consisting of 262 x 530W PV Modules 

	Permitted Development Information
	Solar PV modules must not protrude more than 0.2m beyond the plane of the roof slope when installed on a pitched roof 

Solar PV modules must not protrude more than 1 meter above the highest part of the roof when installed on a flat roof 

The solar PV equipment must not be installed within 1 meter of the external edge of the roof 

Further information can be found at https://www.legislation.gov.uk/uksi/2015/596/schedule/2/part/14/crossheading/class-j-installation-or-alteration-etc-of-solar-equipment-on-nondomestic-premises

	Roof type 
	Pitched Roof Design

	Mounting System type
	Clenergy Standing Seam (additional information below)

	Site / Design Images and Information

	Project Overview
	[image: ]

	Site Location
	[image: ]

	Site Modelling
	[image: ]

	Roof Plan (Including dimensions)
	[image: ]

	Roof Elevation Identification Plan
	 [image: ]1


	Module installation plan (including 1m perimeter)
Elevation 1

Additional images shown in appendix A
	[image: ]
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	Module Dimensions 
	Length - 2063 mm / Width - 1134 mm / Frame Depth - 30mm
[image: ]

	Mounting Dimensions
	    [image: ]

 Finished protrusion height of solar panels above existing roof plane - <0.5m
[image: ]




System Declaration 

I confirm that the above information is true and accurate and that to the best of my knowledge the project specification outlined above satisfies the requirements of the Town and Country Planning (General Permitted Development) (England) Order 2015 (Update 21/12/2023) Class J – Installation or alteration of solar equipment on non-domestic premises.

Signed 


[image: A black letter with a curved edge

Description automatically generated with medium confidence]

Ben Nuttall 
System Designer 
NPS Energy Ltd 
Completion of report 

Appendix A

 [image: A computer screen shot of a computer

AI-generated content may be incorrect.] This image shows the panels are 120cm from external edge A.C
A



 [image: A close up of a computer

AI-generated content may be incorrect.] This image shows the panels are 326cm from external edge B.D
C
B
A





 [image: A screen shot of a video game

AI-generated content may be incorrect.] This image shows that the panels are 100cm from external edge C.C
D
B
A
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 [image: A black and white background with squares

AI-generated content may be incorrect.] This image shows that the panels are 215cm from external edge D.D
C
B
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