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Floor plan 34 Rooley Moor Road.

Windows/Doors (in metres)

	Ground Floor
	Window 1
	Window 2
	Window 3
	Window 4
	Window 5
	Door

	Kitchen
	1.067x0.60
	1.067x0.62
	1.067x0.60
	N/A
	N/A
	1.89x0.97

	Reception Room
	1.48x1.28
	N/A
	N/A
	N/A
	N/A
	

	First Floor
	
	
	
	
	
	

	Bathroom
	1.068x0.627
	1.068x0.636
	N/A
	N/A
	N/A
	N/A

	Bedroom 4
	1.09x0.65
	1.09x061
	N/A
	N/A
	N/A
	N/A

	Bedroom 1
	1.447x1.341
	N/A
	N/A
	N/A
	N/A
	N/A

	Second Floor
	
	
	
	
	
	

	Bedroom 2
	1.024x0.64
	1.024x0.63
	1.024x0.593
	1.024x0.635
	1.024x0.60
	N/A

	Bedroom 3
	1.078x0.607
	1.078x0.646
	1.078x0.644
	1.078x0.619
	N/A
	N/A












Ground Floor

Kitchen Windows 
Window 1 (Right)
1.067x0.60




Window 2 (Centre)
1.067x0.62



Window 3 (Left)
1.07x0.60

[image: A window with a reflection of a person in it
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Kitchen Door
Back Stable Door
1.890x0.970

[image: A door with a window and a potted plant
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Bathroom & Bedroom 4 Windows[image: A building with windows and a pipe
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Window 1 (Right)
1.068x0.650

Window 2 (Left)
1.067x0.640





Bedroom 4
Window 1 (Right)

1.092x0.650
Window 2 (Left)
1.092x0.61



Bedroom 1 WindowBedroom 1

1.476x1.285

(No Central Mullion)

[image: A window with bars on the side of a building

AI-generated content may be incorrect.]

Bedroom 3
Window 1 
1.078x0.607




Window 2 
1.078x0.646



Window 3 
1.078x0.644


Window 4
1.078x0.619


[image: A building with windows on the side
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Bedroom 4
Window 1 
1.0078x0.636


Window 2 
1.067x0.627


Window 3 
1.078x0.593

Window 4
1.078x0.635


Window 5
1.078x0.600

[image: A building with many windows
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Front Door (Size TBC)


[image: A brown door with a stone wall and a planter
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Product Specification

All windows were replaced with Sapele Hardwood and colour-matched to the existing windows. A drawing of large scale cross section has been provided below. All front windows have been replaced with faux leaded as per the originals.. Glazing is 14mm (4/6/4) to comply with the regulations for traditional/heritage DG. Coloured sealant was used rather than cement for pointing purposes. 

[image: ]


Old windows. I have attached copies of the old (1986) windows and UPVC door for reference.
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