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METHOD STATEMENT

Installation of Electricity Service Cable and Cable Guard to Listed Building and Removal of Existing Overhead Service

These works form part of the Maw Rode / Moor Road reinforcement scheme (Project Ref: 60006675), which involves undergrounding an existing span of LV overhead line, removing the existing overhead services to Maw Rode Farm and Maw Rode Barn, and installing a new underground-fed electricity service cable with a protective cable guard fixed to the external wall of the properties with Maw Rode Barn being a listed building.
This method statement details the works involved at Maw Rode Barn. 

Scope of Works
The works involve the removal of the existing overhead electricity service cable to the listed building and the installation of a new underground-fed service cable. The new cable will be fixed to the external wall of the property and protected by a cable guard to approximately 1.8m above ground level. The installation will be carried out in a manner that protects the historic character and fabric of the building.
Personnel and Equipment
Works will be undertaken by competent operatives under the control of a site supervisor. Equipment may include ladders or MEWP access equipment, battery drills, hand tools, cable installation equipment, testing equipment, barriers and signage.
PPE
All operatives shall wear suitable PPE including safety boots, hard hat, hi-visibility clothing, gloves and eye protection.
Method of Work
1. Establish the work area using suitable barriers and warning signage.

2. Confirm permits, approvals and listed building requirements before work commences.

3. Isolate the existing electrical service and prove the circuit dead in accordance with company procedures.

4. Access the building using approved access equipment and carefully disconnect the existing overhead service cable.

5. Remove the overhead service cable and any redundant brackets, clips or fittings.

6. Make good minor fixing holes where necessary and remove all redundant materials from site.

7. Mark out the approved route for the new service cable on the building facade.

8. Install cable clips and supports using appropriate fixings, preferably within mortar joints wherever reasonably practicable.

9. Install the new service cable and secure it neatly to the wall, ensuring compliance with manufacturer requirements and minimum bending radii.

10. Install the cable guard over the service cable from ground level to approximately 1.8m above ground level to provide mechanical protection.

11. Seal any cable entry points to prevent water ingress.

12. Carry out inspection and testing of the new installation before reconnecting the supply.

13. Reinstate the work area and remove all equipment, waste materials and barriers.
Protection of the Listed Building
Particular care shall be taken to avoid damage to the historic fabric of the building. Drilling shall be kept to a minimum and existing fixing locations reused where possible. Any damage identified during the works shall be reported immediately and appropriate repairs agreed before completion.
Health, Safety and Environmental Controls
All works shall be carried out in accordance with current health and safety legislation, site RAMS, Electricity at Work Regulations and Work at Height Regulations. Good housekeeping shall be maintained throughout the works and all waste materials removed from site for appropriate disposal.
Completion
The works shall be deemed complete when the overhead service has been removed, the new service cable and cable guard have been installed, testing has been completed and the site has been left in a clean and tidy condition.
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