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Highways and Engineering Service 
Economy and Environment

Consultation Response on behalf of Head of Highways and Engineering

Application: 25-01018-FUL

Date Received:      24 October 2025

Date of Response: 28 October 2025


Proposal:
Residential development of a 100% affordable housing scheme comprising of one, three storey block of 24 apartments and a row of 6 terraced dwellinghouses, alongside creation of access, landscaping, drainage and other associated works

Consultation Report:
The application site is situated along a narrow lane at the furthest extent of the borough. There are some local amenities in the vicinity and good public transport links to a number of locations.
The traffic generation associated with a residential development of this size is very low. Whilst the increase in traffic will be noticed by neighbouring properties currently at a dead end the traffic volume is not expected to be problematic in terms of function along Waterfold Lane or at the junction with Bury New Road.
The level of parking provided is adequate for a development of this size in close proximity to public transport links.
The proposed site access is a long a quiet lane with shuttle working proposed along the narrow sections. The potential for traffic moving in conflicting directions along this route is very small due to the low volume of traffic generated. This is an acceptable arrangement and should keep vehicles speeds down on this ‘quiet lane.’
There is no additional changes to the existing highways network proposed as a result of this development.
No new highways are proposed as part of this proposal
No PROW will be obstructed by this proposal.
We have no new road safety concerns as a result of this proposal.
Refuse collection and servicing from this location should not be problematic.
Amendments to Consultation Response:
No amendments to report
Officer Recommendation:
We have no objections to this development as proposed.
Highways Sign off
John Gillighan 28/10/2025
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