Proposed agricultural building, Long Clough Farm, Clough Road, Littleborough OL15 9PA

Landscaping Plan
Ref: AG.030625
Areas  shaded green to be planted with trees in accordance with the BNG submission


[image: ]Existing hardstanding around the proposed building to be retained. 



Tree planting
Planting details
All planting operations shall comply with BS 4428 (1989) & AMD, Code of Practice for General Landscaping Operations
•	Total minimum soil depths: 150 mm topsoil, minimum 300 mm subsoil 
•	Subsoil shall conform to BS 8601:2013 Specification for Subsoil and             requirements for use.
•	Topsoil conforming to B.S. 3882: 2015 shall be multi-purpose soil of uniform composition throughout, of light to medium texture, and shall be capable of being broken down to a fine tilth.
Planting to be contained within 900mm high wooden post and 2-rail fencing

Amount
A minimum of 28 small trees to be planted within the areas coloured green on the above plan and in accordance with the BNG documents submitted with the planning application. 

Species and sizes

	%
	Botanic
	Common
	Nursery size

	50
	Crataegus monogyna
	Hawthorn
	Min 750mm 

	50
	Prunus spinosa
	Blackthorn
	Min 750 mm



Maintenance
Any plants failing within first 5 years to be replaced by same
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