ENVIRONMENTAL CONSTRUCTION METHOD STATEMENT
SITE

Kirkway Service Station Middleton M24 1LW
PROJECT
Construction of New 5No Dwellings (2 Pairs of Semi-Detached and 1No Detached)
DUST
The contractor is committed to minimising dust emissions. The main cause of dust within a site is the use of ‘disc cutters’ and similar machinery for cutting blocks and stone etc. These machines will be fitted with a hose to dampen the dust emissions. The site will also have a hose pipe continually available to dampen down any areas of dust build up to ensure the spread is minimised. Any hardstanding areas will be constantly dampened and swept to reduce the dust emissions.

Vehicles will also be washed if appropriate to ensure dust is not transported from the site from wheels etc.

MIGRATION TO RESIDENTIAL PROPERTIES
The site boundary is adjacent to the rear gardens of residential properties. The migration of construction material to these is a small risk. However the entrance to the site is 10m from these boundaries and therefore a wheel wash facility will be available for all vehicles leaving the site.

WORKING HOURS
As stipulated in  the planning 8.00-18.00 Monday to Friday, 9.00-16.00 Saturday and no working on Sundays and Bank Holidays.
SITE SECURITY
The site will be fenced with steel herras fencing with a secure gated entrance utilizing the existing access. Delivery vehicles will enter the site for unloading and will report the site manager.

SKIPS
All site skips will be enclosed to avoid the possibility of material being blown off site.

SITE STORAGE
All materials will be stored in security compounds.
The site compound and Welfare Facilities will be situated on the site of Plot .5.
CONCRETE MIXING
A concrete batching and mixing area will be set up at the furthest point from the residential boundaries to ensure no migration to these properties.
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