Please quote 27637-7151-PL1 in all correspondence.

Please note that advance approval is required before a site visit – even if the visit is only to the outside of 
the branch. Due to heightened awareness of criminality around bank branches staff will spot and report 
incidence of suspicious activity to the local constabulary. 
To avoid any undue interaction with the police please call us on 01142490944 to arrange a visit. Three 
working days’ notice is required to ensure the visit can be arranged with all internal parties. 
If you have any queries about a visit to a site, please email richard@axis-architecture.com or call 
07912731638.
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Site Address: 
HSBC UK Bank plc,
2 Yorkshire Street, 
Rochdale, 
Lancashire, 
OL16 1EE

1.0	Introduction

1.01	This Flood Risk Assessment has been produced in support of the planning application to replace section of high level roof covering to front area of building at HSBC UK Bank, Rochdale.

2.0	Development Site 

[bookmark: _Hlk519868674]2.01	The bank is located on Yorskhire Street, in the centre of Rochdale and in close proximity to an exposed section of the River Roch.

3.0	Development Proposals

3.01	The proposals can readily be broken-down into the following components which form the focus of this assessment: 

I. Replacement of 1no. external ATM machine

3.02	No new floor area will be added to the building as part of this proposal. All existing floor levels, access and escape routes and surface water management measures will be unaffected.

4.0	Sequential Test

4.01	As the proposed development is a very minor addition to an existing building, the Sequential Test does not apply. 

5.0	Exception Test

5.01	As the proposed development is a very minor addition to an existing building, the Exception Test does not apply. 



6.0 	Site Specific Flood Hazards

6.01	As the site is located in close proximity to the River Roch in a heavily paved area of town, the most likely flood hazard to the site is fluvial flooding due to channel capacity being reached, as per historical floods (please refer to Appendix B.) 

7.0 	Flood Risk Management

7.01	The ground floor of the existing building is raised above street level, affording it some extra protection in case of the river bursting its banks. 

8.0	Conclusions

8.01	As the proposed development is for roof covering replacement to prevent the ingress of water, we do not believe that the proposal will increase the risk of flooding to the existing bank and infact further protect the building from water ingress. 
 


Appendix A
Flood Map denoting local Flood Zones and Site Location
Source: Environment Agency


Appendix B
Flood Risk Assessment Data
Source: Environment Agency

