Anti-vandal rollers

[image: C:\Users\rigghamish\AppData\Local\Microsoft\Windows\INetCache\Content.Word\IMG_0208.jpg]‘vangard’ Single roller barrier (Colour: black) fixed with a cranked support bracket in galvanised aluminium 25mm support shaft.

Vandgard Roller Barrier – Vandgard® - Anti Climb Guards Ltd
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