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[bookmark: _bookmark2]Existing infrastructure
Records received from Openreach show:
· [image: ]Existing Openreach apparatus and associated chambers are present along Trub Road, Rochdale



· Risk assessment
Disconnections
No disconnections are required across the site



Figure 1 - BT Openreach infrastructure is present at the site.
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· [bookmark: _bookmark3][bookmark: _bookmark4]Utility Depths
The National Joint Utilities Group (NJUG) are an industry-recognized non-regulatory body that provide guidance on new utility infrastructure and construction.  The recommended minimum depth for Comms apparatus, as per NJUG guidelines, is as follows:
»250mm – 350mm in footway/verge.

Figure 2 - NJUG Detail

New connections
Fibre to the Premise enables superfast broadband to be delivered directly into a property. Fibre is run from the local exchange, terminating in a cabinet.
From here, fibre lines connect each property to the cabinet to provide superfast speeds.
Openreach give access to a multitude of Internet Service Providers (ISP) within their network, allowing a variety of options to the end occupants of the buildings in terms of who can supply their internet.


[bookmark: _bookmark6]We would typically Install BT Openreach to all our sites as a main service but in this instance, there is also Virgin Media available as a secondary comms supplier to provide resilience to the site and more options to the end occupants of the building in terms of the internet service providers available to them. 

	TELECOMMUNICATIONS –
VIRGIN MEDIA
Existing infrastructure
•Virgin Media apparatus and associated chambers are present along Trub Road, Rochdale

· Risk assessment
Disconnections
No disconnections are required across the site





· Utility Depths
The National Joint Utilities Group (NJUG) are an industry-recognized non-regulatory body that provide guidance on new utility infrastructure and construction.  The recommended minimum depth for Comms apparatus, as per NJUG guidelines, is as follows:
»	250mm – 350mm in footway/verge.
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[image: ][image: ]figure 3 - Virgin Media infrastructure is present at the site


Figure 4 - NJUG Detail

New connections
To procure Virgin Media MCI Developments Ltd will need to register the site and submit a  formal enquiry to provide new connections to the site. This would provide an alternative fibre option to Openreach. 



Local Internet Speeds- 

[image: ]An internet speed search for Cale Lane, Wigan shows that the standard download speed for this area is – 67.8Mbps. Superfast Broadband is also available.  The UK average download speed is between 50.4 and 79.1Mbps meaning that the site towards the upper threshold of the UK average therefore ample internet speed is available for most homes utilizing the internet for normal requirements such as TV, internet, and gaming. 





 Figure 5 - Speed Map
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