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BS 5837:2012 advises that in order to provide adequate protection from building interference, a building should be at least 1m beyond the canopy of a tree or 12 times its diameter whichever is greater.
In this case the trees as shown on the attached plan, as measured on site and at chest height, have similar circumferences of between 1.4metres and 1.45metres Using the higher figure, that equates to a diameter of 0.46 metres
Thus, the proposed agricultural building should be 5.5 metres away.
But in addition, a 20% reduction in the root protection area is regarded as suitable if the tree has unrestricted roots on one side of the tree.
Such a reduction gives a distance for a root protection area (RPA)  of 4.6m
The proposed building has been re-positioned to be a minimum of 5.5 metres away from the nearest  trees with the above circumferences /diameters.  
As such, the building would also be at such a distance from the hedging adjoining the lane.
In addition, we propose to erect heras fencing at a minimum distance of 4.8m from the boundary hedge and trees to give added protection during construction. 

Within the protected area there none of the following will be permitted: -
1. No ground disturbance or excavations
2. No storage of materials or chemicals
3. No burning of materials
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