Planning Approval reference 24/00349/HOUS
25 Hurstead Road
Milnrow
Rochdale OL16 3JS
Discharge of Condition 3
Details of materials to be used externally 

1 External walls to be Carlton Heather Sandface 73mm to match the existing house. A band course from ground level to DPC level of red faced engineering bricks to be incorporated to match the existing house. 

2 The roof is to be Marley Monarch tiles to match the original house.
3	New widows and doors are to be Anthracite coloured uPVC to match the existing. 
 
  
 








