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MATERIAL SCHEDULE	

[bookmark: _Hlk54352430]SITE ADDRESS		10 GREENMOUNT DRIVE, HEYWOOD, OL10 2LZ
			
CLIENT			MS STEPHANIE MOSS

DATE			DEC 2022

REVISION		-

STAGE			BUILDING REGULATIONS
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[image: A hand pointing at a brick wall

Description automatically generated with low confidence]Main Facing Brick
Terca Weathered Sandblast 

(Proposed brick being held against existing brick)


[image: Western Red Cedar No. 2 Clear & Better Channel Cladding | Silva Timber |  Silva Timber][image: Japanese Burnt Cladding - Yakisugi - Shou Sugi Ban][image: Marley Ludlow Major Interlocking Concrete Roof Tile Antique Brown - Pallet of 216]



Shou Sugi Ban Timber Cladding











Cedar Timber Cladding












Marley Ludlow Major Interlocking Concrete Roof Tile
(Antique Briwn)





[image: Benefits of pre-coated aluminium cladding | Proteus Facades]



Aluminium Rainscreen Cladding
(Protues Anthracite Grey Pre-coated system)
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